# MOWING (SPECIAL)

Revised: 9/28/2017

**Description:** This work shall consist of mowing all grassed, turfed, and/or temporary seeded areas within the project right-of-way limits to keep floral resources from blooming, or as directed by the Engineer. The equipment used shall be capable of adequately mowing all areas surrounding existing trees and shredding all regeneration of brush 2 inches in diameter or less to the satisfaction of the Engineer. Mowing shall be completed weekly, between March 15th and October 14th. The mowed area(s) shall be no greater than approximately 3-inches in height or as approved by the Engineer.

**Method of Measurement:** Each mowing occurrence will be paid for separately.

**Basis of Payment:** This work shall be paid for at the contract unit price per acre for MOWING (SPECIAL), which price shall include all labor, material, and equipment necessary to complete the work described above.