# POLYMERIZED HOT-MIX ASPHALT BINDER COURSE

Created: 1/17/2024

This shall be done in accordance with **section 406** of the Standard Specifications insofar as applicable and the following provisions:

The limits, mix type, and thickness for this work are shown on the location maps, the schedule of quantities, the typical sections, and as directed by the engineer. The mix types will have the following properties:

MIX VOIDS

Polymerized Hot-Mix Asphalt Binder Course, IL-4.75, N50 3.5% @ 50 Gyr

All calculations involving unit weights shall use 110 lbs./sq. yd./in.

All paving operations shall be performed to minimize impact to traffic flow. Therefore, only one mainline through lane may be closed for paving operations at any time.

**Basis of Payment:** This work shall be paid for at the contract unit price per ton for POLYMERIZED HOT-MIX ASPHALT BINDER COURSE (MACHINE METHOD), of the mixture composition and Ndes specified, which price shall include furnishing and placing of binder course and all materials and labor necessary to complete the work described above.