# BREAKAWAY DEVICE *(Kane Co. Supplement)*

Updated: 01-01-2023

Revise Article 1070.04(b)(2) of the Standard Specifications to read:

“The devices shall be approximately 9 in. (230mm) high and shall have a large fiberglass or polyethylene access door and a color to match the base finish which shall be held in place with a button-type tamper resistant stainless-steel screw or other means approved by the Engineer.”