# MAST ARM SIGN PANELS *(Kane Co. Supplement)*

Updated: 09/15/2023

This specification is intended to supplement the IDOT special provision 720.01 TS for Kane County Projects. In places of Conflict, this specification shall supersede:

Add the following to Article 720.02 of the Standard Specifications:

Sign stiffening channel systems shall be aluminum and meet the requirements of ASTM 6261-T5. Sign mounting banding, buckles and buckle straps shall be manufactured from AISI 201 stainless steel.

Add the following to Article 720.04:

(c) any Traffic signal structure; such as a post, pole, mast arm or pole or any other traffic signal structure, regardless of the size of sign.

(d) mast arms, where a sign panel is used as a dampening plate.