# SIGN face, sign legend, and supplemental panels *(Kane Co. Supplement)*

Updated: 09/15/2023

Revise the second paragraph of Article 1091.02 the Standard Specifications to read:

Signs shall be fabricated such that the material for the background, legend, border, shields, and symbols are applied in the preferred orientation for the maximum retroreflectivity per the manufacturer’s recommendation. **A graffiti film shall be installed protecting the sign face and sign legend and shall be manufactured from the same manufacturer of the sign face background and background material.** When using Type ZZ retroreflective sheeting, the nesting of legend, border, shields, or symbols will not be permitted.