TRANSVERSE RUMBLE STRIPS

Revised: 1/27/2017

This work shall consist of milling transverse grooves (as detailed in the Transverse Rumble Strip detail) from the centerline of the mainline to the outside edge of pavement in the direction of traffic approaching a controlled stop intersection, at locations indicated in the plan improvements, or as specified by the Engineer.

The recommended placement and configuration of the transverse rumble strips should be three groupings of strips 8 inch (200mm) wide separated by 4 inch (100mm); milled into the surface of the pavement.

**Basis of Payment:** This work shall be paid for at the contract unit price per square yard for TRANSVERSE RUMBLE STRIPS, which price shall include all labor, material, and equipment necessary to complete the work described above.