TREE REMOVAL

Revised: 1/26/2017

This work shall consist of the complete removal and off-site disposal of existing trees and bushes as shown on the site plan. Trees shall be removed in a safe manner in accordance with best practices and recognized methods. Care shall be taken not to damage adjacent structures and/or foliage during the removal process. Tree stumps shall be removed in their entirety where possible. Grinding of large tree stumps will be permitted providing stumps are ground to at least 3 feet below grade. Holes from tree removal shall be backfilled with Type a granular CA-06 material compacted to 90% modified density and placed in 6” loose lifts. Final grade shall match the surrounding contours and the adjacent areas seeded with rapid growing quality grass seed as applicable.

**Basis of Payment:** This work shall be paid for at the contract unit price per each for TREE REMOVAL, which price shall include all labor, material, and equipment necessary to complete the work described above.