# MAINTENANCE OF ROADWAYS / TRAFFIC CONTROL DEFICIENCY

Revised: 3/16/2023

Beginning on the date that work begins on the project, the Contractor shall assume responsibility for normal maintenance and/or any damage of all existing roadways within the limits of the improvement. This normal maintenance shall include all repair work deemed necessary by the Engineer, but shall not include snow removal operations. This shall include pot holes which may develop, after milling of the roadway, while the roadway is left open before paving operations begin.

Traffic control and protection for maintenance of roadways will be provided by the Contractor as required by the Engineer.

The Contractor shall commence work on all maintenance of roadways items within 2 hours of discovering such items or within 2 hours of notification by the Engineer and shall complete such items in an expediant and timely manner. Failure to do so may result in a ***deficiency of $2000 per calendar day***.

If items of maintenance work have not been provided for in the contract or otherwise specified for payment, such items, including the accompanying traffic control and protection required by the Engineer, will be paid for in accordance with Article 109.04 of the Standard Specifications.

Basis of Payment: This work shall be paid for at the contract unit price per lump sum for TRAFFIC CONTROL AND PROTECTION (SPECIAL), which price shall be payment in full for all labor, materials, and equipment necessary to complete the work described above.