# TRAFFIC BARRIER TERMINAL, TYPE 1 (SPECIAL) TANGENT

Revised: 9/14/2022

**Description:** This work shall consist of furnishing and installing Traffic Barrier Terminal Type 1, Special of the type specified by the Engineer from the approved IDOT qualified products list of Traffic Barrier Terminal, Type 1 Special, according to Section 631 and the following:

All terminals shall meet the testing criteria contained in AASHTO Manual for Assessing Safety Hardware (MASH) and be approved by the Engineer.

The terminal shall be installed according to the manufacture’s specifications and shall include all necessary transitions between the terminal and the item to which it is attached.

The terminals shall follow the manufacturer’s specifications for installation as to the type and number of posts, foundation tubes, and soil plates.

**Basis of Payment:** This work shall be paid for at the contract unit price each for TRAFFIC BARRIER TERMINAL TYPE 1, (SPECIAL) TANGENT, which price shall include all labor, material, disposal of excavated material and equipment necessary to complete the work as described above.